DAMAGES:-
1. Front Cowl Assy. The front cowl assy. of the vehicle totally damaged along with its internal parts.
2. Cabin:- Cabin of the vehicle totally broken/damaged.
3. Chassis Assy.:- Chassis Assy. of the vehicle totally bent/twisted at its front side. Upto approx. 8 feet length not repairable (U- Shaped)
4. Cooling System:- The cooling assys. i.e, Radiator, inter-cooler, fan and all its connected assy. totally damaged. 
5. Electrical Systems:- All the electrical system wiring, sensors, battery, wiring front, engine controlling system, electric control Module etc. broken, meter panel broken.
6. Braking System:- Braking System, pipes, control broken. Master cylinder, damper etc. broken.
7. Front Suspension System:- Both side Spring leaves assy. bent, tie rod end sets and there connected parts bent/de-aligned. Front under assy. de-aligned.
8. Rear axle assy:- Rear Axle assy. needs check. Spring leaves bent/de-aligned. 
9. Load Body:- Both side walls of load body bent, lars broken at the front side. Angles bent due to impact of falling and the pressure of load developed at the time of fall. Iron sheet & angles bent. Vertically & horizontally also complete load body needs dismantling & new fabrication.
10. Engine Assy. The engine assy. dislocated/shifted backwardly. Front portion of engine assy. pressed. Fuel pump, alternator, self, diesel pipes and other connected parts needs check. Engine foundations broken. Oil Sump dented; silencer assy. dented/pressed. Water Pump; Engine Pulley broken. 
11. Gear Box:- The gear box assy. broken and fallen/lying on the ground. Gear lever assy. broken; Gear foundation broken. Gear shaft broken; Front propeller shaft broken & lying on the ground.
12. Both the propeller shafts de-aligned.
13. Diesel tank dented, pipes bent/twisted.
14. Brake & air pipes broken.  
15. Urea container tank and its upper unit (Doser Pump Unit) broken/damaged.

