DAMAGES:-

1. The impact of the collision is so high that the engine/gear box assy. is shifted backwardly by about 1 feet after breaking the engine foundation & gearbox foundation. It is also possible that engine block & other parts which are connected with the engine/gear box have damaged which could be came to for-seen when the vehicle is dismantled for repairs. 
2. Radiator & Condenser, shroud fan etc. damaged.
3. Head lights; parking lights; fog lights broken.
4. Front tie member damaged.
5. Bumper, grills and other plastic parts fixed in the front of the vehicle are damaged.
6. Air Cleaner broken.
7. Battery Broken. 
8. Both side front suspension damaged.
9. Air bags actuated and their modules damaged.
10. Fender L/S Bonnet center; Apron both sides badly dented & twisted.
11. I may add that the welding of the Apron assy. with the dash panel is uprooted/broken.
12. Front suspension bracket/bent.
13. Wiring cut/broken.
14. Steering rack assy. seems damaged.
15. AC Pipes bent/torn/pressed.
16. L/s door buldged out badly.
17. Dash board/instrument panel cracked.
18. Rear Bumper broken.
19. Rear R/S Qtr. Panel dented.
20. Engine oil leaked as shall be visible on the ground. 
21. Exhaust manifold cracked.
22. Front portion of silencer assy. bent. 
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