EXTERNALLY VISIBLE DAMAGES:

1. Cabin/Load Body:- Cabin of the vehicle badly damaged. Both side Al. Fittings; internal wooden work; upper tool box; front W/S glass; cabin side glass; cabin back side – damaged/broken. Both side of load body badly bent; Lars broken/cracked; angles bent.

2. Cowl assy./show – badly damaged. Cowl assy. frame bent/twisted. Dashboard bent. Welding of cowl assy. uprooted at different places. 

3. Engine of the vehicle reported damaged. Engine Block seems broken at places – To check after dismantling the vehicle.

4. Battery acid/water leaked cracked.

5. Wiring damaged/cut.

6. Front suspension assy. & Chassis frame bent.

7.	The above are the externally visible damages and there is possibility that some other damages/internal damages which became apparent on dismantling shall be taken into account. Keeping in view the nature/cause of accident.  


PLEASE QUOTE YOUR VALUE WITH R/C AND WITHOUT R/C – BOTH


 
