EXTERNALLY VISIBLE DAMAGES:
Cabin	:-	Cabin of the vehicle totally broken & uprooted, both sides of cabin damaged, front glasses broken; R/S & L/S totally broken. Cabin back side also broken. Cabin is totally broken. New Cabin to be fabricated. Both Rear doors dented/twisted. 

Container	:-	The container body sheets, upper bent & torn. Right side sheets bent/dented. L/S Sheets dented/bent & torn. Lower floor of container de-aligned as the chassis frame is bent completely. New container is to be fabricated. 

Chassis Frame	:-	Chassis frame of the vehicle totally bent at the centre – as visible in the photos attached. 

Front Suspension:-	The vehicle has rolled down on the hill surface over big boulders. The front axle, tie rod etc. needs check for any de-alignment/bent.

Rear Suspension:-	The vehicle has rolled down on the hill surface over big boulder. The Rear Differential tube has hit the boulders, needs check at the time of repairs.

Propeller Shafts:-	All the propeller shafts bent.

Battery	:-	Two Ni. Batteries are broken.

Diesel Tank	:-	Diesel tank totally dented/bent, one side of the tank came out after breaking the welding.

Suspension Assy:-	All the leaf springs assy. seems intact, however the same needs check.

Wiring	:-	broken/damaged.

Cowl Assy.	:-	The cowl assy. of the vehicle was sustained impact. Front cowl sheets dented, its alignment may be effected, as the vehicle has rolled down and the cabin is uprooted from the front side (as visible in the photos).

The above are the externally visible damages and there is every possibility that some other damages may came to light when the vehicle is dismantled for repairs, which shall be taken into a/c keeping in view the Nature of loss.   

