DAMAGES:-
1. Front W/S glass broken, glass frame bent.
2. R/S Front door frame bent.
3. R/S Front Fender; Apron Assy. Bonnet centre; Front member dented/bent/twisted.
4. Front Bumper broken.
5. R/S Front Wheel Rim bent/twisted & tyre flattened. 
6. Instrumental panel broken.
7. Steering wheel bent & column bent
8. HAVC unit broken.
9. Meter Panel broken – wiring cut/broken.
10. Radiator & Condenser Assy. bent/pushed back
11. Front Grills broken.
12. AC Pipes bent/broken.
13. R/S Suspension Assy. bent/strut; axle; arm bent.
14. Roof dented.
15. R/S Body panel dented/bent at the centre.
16. Head lights both side broken.
17. Brake booster damaged.
18. Horn damaged.
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