DAMAGES:-

1. Body Shell:

	a) Front Bonnet and L/s & R/s fenders dented.
	b) Dicky Badly Dented
	c) Both side quarter panel/ body panel dented along with their inner members.
	d) Body dented/twisted at rear side.
	e) Both rear L/s & R/s  doors dented their glass frames bent.
	f) Dicky lower panel pressed inwardly
	g) Both side apron assemblies dented their front edges bent.
	h) Front tie member upper/lower panel dented/bent.
Since major portion of sheet metal portion of body shell is damaged/bent/twisted and they are to be replaced after cutting and rewelding, It appears that car has fallen on its back side and then on the front side, due to which both the back side & front side of the car are damaged (as can be seen from the photos attached) as such new body shell is allowed.

2) Rear Dicky glass broken.

3) L/s & R/s rear door glass broken.

4) Radiator condenser pushed back

5) Rear upholstery and roof upholstery.


PLEASE QUOTE YOUR BIDS WITH & WITHOUT R/C – BOTH. 
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