EXTERNALLY VISIBLE DAMAGES:-
1. Front Bumper – damaged/bent at L/S.
2. Fender L/S – damaged/dented.
3. Door Front L/S – damaged/deshaped.
4. Door Rear L/S – damaged/deshaped.
5. Qtr. Panel L/S – Damaged/Deshaped.
6. Rear Bumper – damaged/deshaped
7. Dicky – damaged/dented.
8. Roof – damaged/deshaped.
9. Qtr. Panel R/S damaged/dented.
10. Rear Door R/S – Damaged/dented.
11. Front Door R/S damaged/dented.
12. Windshield Front – Damaged/broken.
13. Windshield Rear – damaged/broken.
14. L/S Wheel Rim – damaged/broken.
15. Body Panel L/S badly damaged along with central member,
16. Floor of the car, dented/bent/twisted on L/S.
17. The body shell of the car is damaged to such an extent that it is not practically possible to repair the same for which reason new body shell is allowed.
18. Door Glasses broken.
19. Internal door & roof upholstery damaged. 
20. Door internal fittings like glass, machines, handles & other levers bent/twisted.
21. Dash board/instrumental panel broken. 
22. The above are the externally visible damages & there is every possibility some other damages may came to light as & when the vehicle is dismantled for repairs. 

