DAMAGES:-
1. Body Shell:- Since most of the metal parts of body shell are damaged & keeping the extent of damage in consideration new body shell is allowed, which please note 
2. Roof damaged/bent.
3. Bonnet damaged/dented.
4. Windshield front damaged/broken.
5. Fender R/S damaged/dented. 
6. Door Front R/S damaged/dented.
7. Door Rear R/S damaged/bent.
8. Quarter Panel R/S – damaged/bent.
9. Tail Gate – damaged/bent.
10. Quarter Panel L/S damaged/dented.
11. Door Rear L/S damaged/dented. 
12. Door Front L/S damaged/dented.
13. Fender L/S – damaged/twisted. 
14. Pillar Front & Rear damaged/broken.
15. Bumper front & Rear damaged/broken.
16. Windshield Rear broken.
17. Head Lamp R/S & L/S broken/damaged.
18. Apron R/S damaged/bent.
19. Tail Lamp R/S & L/S – damaged/broken.
20. Dash board broken/cracked 
21. Air bags – damaged/actuated. 
22. Seat belts are actuated. 
23. ABS brake system damaged.
24. Air Cleaner broken.
25. AC Pipes bent/pressed.
26. R/S Suspension assy. damaged. R/S wheel rim bent; shocker bent.
27. Front Grills broken.
28. Radiator & condenser pressed pushed back.
29. Fan shroud assy. broken.
30. Steering wheel de-aligned. 
31. Roof lining & inner upholstery damaged.  

