EXTERNALLY VISIBLE DAMAGES:

1. Front W/S glass broken; Wiper blade & arms bent.
2. Roof Glass broken.
3. Front glass both pillar bent.
4. Sheet metal portion of roof dented.
5. Bonnet centre dented & deshaped. 
6. Dash board & instrumental panel scratched. 
7. Both front air bags actuated – modules actuated. 
8. R/S Front door dented.
9. R/S Rear view mirror broken.
10. R/S Front door glass broken; Weatherstrips bent.
11. R/S Front Fender dented. 
12. Front Deflector panel – plastic broken.
13. Front Bumper broken. Fog lights broken.
14. Other plastic linings broken.
15. Both head lights broken – fastening clips broken.
16. Left side front fender dented.
17. Rear View mirror L/S broken.
18. Front door dented & handle broken on Left side. 
19. Rear Door dented – L/S
20. Rear Qtr. Panel dented – L/S
21. Rear Bumper clips broken.
22. Rubber/Plastic mouldings of door damaged.
23. Door Plastic strips bent. 
24. Inner parts viz. glass winding machines bent.
25. L/S Front door glass broken.
26. Front Grill broken.
27. Front R/S Wheel Alloy scratched/bent.
28. Right side Front Apron assy. bent at front edge
29. R/S Front Suspension Assy. needs check.
30. Front Tie member bent at right side joint with apron assy.
31. Roof Lining broken.
32. Roof Glass broken and their side frames also bent/damaged.
33. Radiator/Condenser assy. needs check.
34. Right side front tyre brusted – The vehicle hit the foot path due to which R/S suspension and other parts seems effected – needs check. 

The Front side of the vehicle was lifted with the crane inorder to check the under-chassis assys. Following main parts were found bent/broken.

1. Steering Rack assy. broken.
2. Right side long member of chassis frame extensively bent.
3. Suspension arms bent.
4. Tapet Cover(Plastic broken).
5. Sensor damaged. Plastic/rubber pipe broken.
6. Right side Apron assy. bent/twisted.  

