THE DAMAGES SUSTAINED BY THE VEHICLE.
1. Front W/S glass cracked.
2. R/S Fender badly dented & deshaped.

3. R/S Front Pillar of Dash Board bent.

4. Cowl top panel dented at R/S

5. R/S Apron assy. bent & pushed inwardly.

6. R/S Wheel Rim (alloy) – bent/cracked at inner side.

7. Front Bumper broken.

8. Bonnet Centre dented/deshaped along with hindges.

9. Engine covers broken.

10. Head Lights both sides broken.

11. Front tie member broken (upper side) & lower side bent.

12. Engine mountings & Brackets broken.

13. R/S Front Twisted indicating the inner worm and support system bent/twisted.

14. Lower cross-member bent.

15. Tapet cover broken and some parts also hit the cam shaft which got scratched as per depicted on the photograph.

16. Front Catholic converter assy. (fixed) with mani-fold damaged.

17. Wiring cut/broken.

18. Wiper arms bent.

19. Wiper motor needs check.

20. Pump assy. power steering broken.

21. Tubes carrying power steering oil damaged.

22. Radiator & condenser assy. bent/twisted.

23. Radiator shroud broken.

24. Instrumental panel fastening clips broken.

25. Steering wheel bent/twisted.

26. Radiator grill broken.

27. Timing belt and its cover broken.

28. Alternator pulley bent – needs check.

29. A.C. Compressor pulley – bent – needs check.

30. Oil Sump dented.

31. L/S Fender assy. dented at the upper side.

32. Power Steering oil container broken.

33. R/S Knuckle, shocker, bearings needs check.

34. Indicator lights/Fog lights broken.

35. Wheel Guards broken (Both sides)
36. Sensor assy. for engine and other parts needs check.

37. Fuel filter assy. broken.

38. Link Assy. front stabilizer bar bent.

39. Brake Booster body dented.

40. Master cylinder brake broken.

41. Brake Pipes bent.

