DAMAGES:-
I inspected the above said vehicle & following damages were noted externally:-

1. Cabin totally damaged, the impact of collision has also caused the iron sheets of the load body to bent at the centre, cabin & load body needs totally dismantling/dismembering for repairs.

2. Cowl assy. totally crumbled/damaged, beyond repairs.

3. Steering wheel, steering rod, bracket, steering bracket, U.J. Cross etc. bent.

4. Steering box main shaft broken. All the lubricants pipes broken/bent.

5. Electric wiring broken.

6. Wiper arms/blades bent/broken. Wiper motor broken/bent.

7. Radiator, inter-cooler assy.; fan; fan viscose; fan belt; shroud; Radiator frame bent/twisted.

8. Engine shifted backwardly. Engine foundations & Radiator foundations; Gear box foundation needs check.

9. Chassis assy. bent/de-aligned.

10. Inner engine bonnet assy. cracked.

11. The above are the externally visible damages and any other damages noted after dismantling shall be informed accordingly.

