DAMAGES:-	

1.	Body Shell:- Front Bumper damaged; Bonnet Centre dented; Fenders dented; roof dented & pressed inwardly; R/S doors & Qtr. Panel dented; Dicky dented; Left side doors dented & glasses frames bent; Qtr. Panel dented; Both side body panels dented & pressed inwardly. The alignment of whole body shell is damaged. It may not be feasible to cut both side body panels along with their inner pcs. and to re-weld the same. Since major portion of the body shell is damaged as such new body shell is allowed:-
2.	Front W/S Glass & Rear Glass broken.
3.	Three door glasses broken, their locks & handle are damaged. Inner fittings damaged.
4.	Roof upholstery & inner trims broken.
5.	Dash board scratched/damaged.
6.	Radiator & Condenser assy. pressed inwardly.
7.	Shroud/fan assy. broken.
8.	Rear Bumper inner holding brackets broken.
9.	Both head lights broken.
10.	Wiper arms/blades bent.
11.	Rear View mirror L/S & R/S broken.
12.	Front Two wheel rims bent & their tyres cut.
13.	Engine foundation broken/deshaped, as the engine assy. is found displaced for its position.
14.	A.C. Pipes bent/cut/pressed.
15.	Engine oil was seen leaked (as is visible in the photo attached)
16.	As the vehicle has moved on road divider, as such the lower suspension assy. parts viz, shockers, steering arms; linkages; drive axle may be damaged which can be judged only after opening the vehicle.
17.	Front Suspension frame de-aligned. 		
 
