1.	Body Shell/Chassis Frame:-

The Body Shell of the vehicle is totally damaged/pressed/deshaped at the back side. Back side doors dented/bent. L/S of the shell bent/twisted. Right side bent/twisted. Roof bent/twisted. Floor of the vehicle is bent/twisted at the back side. The chassis frame which is welded along with the body shell is bent/twisted (as is visible in the photos attached). Passenger seat rear most bent, Central seat bent; Front W/S glass broken. Rear door glasses broken; L/S Glasses broken & R/S Rear Glass broken. Upholstery broken/damaged. I may add that since the chassis frame and floor of the vehicle is damaged to such an extent that in my opinion the body shell is not satisfactory repairable.

2.	Spring leaf assy. R/S Rear damaged, the suspension is seen twisted/bent.
3.	Bonnet Centre dented.
4.	Front Grill broken.
5.	Rear Differential tube bent.
6.	Instrumental Panel broken.
7.	Front & Rear bumper broken.
8.	Head Lamps broken.
 
