DAMAGES:-

The Front side of the vehicle is badly damaged, pushed back extensively, thereby causing damages to the front side badly.

1.	The front side pushed back due to which all the plastic parts viz. Bumper; Grills, head light; fog lights & indicator lights are broken.
2.	Front tie member pressed/bent
3.	Bonnet assy. with lock, level & hinges dented/bent.
4.	Radiator assy. condenser assy. & their shrouds bent/broken.
5.	Front Cross-member bent.
6.	H-Frame bent.
7.	Front W/S glass broken; Wiper arms blade bent; wiper linkages bent.
8.	The engine of the vehicle is pushed back. The turbo assy; air cleaner broken.
9.	Wiring cut/broken.
10.	Battery broken. Battery leads cut.
11.	Steering wheel bent/broken. Steering column bent.
12.	Dash bent/instrumental panel broken. Inner parts fixed at the back side seems broken/crumble. 
13.	Front Suspension assy. needs check.	
14.	Alternator & AC Compressor assy. seems damaged, as the engine is pushed back & fallen.
15.	Fuse box broken.
16.	Both side front doors bent & de-aligned.
17.	Roof at front side dented/pressed.
18.	Horn pressed & fallen.
19.	Front both seats (Driver & Co-passenger) bent.
20.	Engine foundation broken and the engine assy. has fallen from its foundation. As the front side is pressed badly, Engine/gear box assy. seems damaged. However the damage to the same can be checked thoroughly on opening the front side.
21.	Both side apron assy. bent; sheet wrinkled.
22.	Power steering bottle broken. Power steering assy. damaged/broken. Steering rack assy. broken.
23.	A.C. Pipe pressed/damaged.
24.	Inter-cooler assy. pressed/damaged.
25.	Catalytic converter pressed/damaged.
 
