1.	Complete Body Shell heated, burnt and damaged. The strength of the body shell sheet is damaged/tempered due to heat generated due to fire & water thrown on it by fire brigade tender. The body cannot be used for the vehicle and it needs replacement.
2.	All the Al. Parts viz. Radiator; Condenser; inter-cooler damaged/partially melted. The other Al. Parts viz. Tapet Cover; Alternator etc. are found melted.
3.	All the plastic/rubber parts; Bumpers; grills; hose pipes; wiring; fuses; head lights; tail lights; combination lights; inner upholstery; seats (driver & co-passenger); rear side; trims; roof upholstery & rear view mirrors burnt.
4.	All the glasses broken.
5.	Weather-strips; door rubbers etc. burnt.
6.	Battery burnt.
7.	Engine assy. Fan cover and other connected parts burnt/damaged. Engine assy. heated. 
8.	Front Suspension assy. heated/de-aligned. 
9.	Front Both side tyres burnt; Wheel rim heated.
10.	Rear Tyres partially burnt and wheel rim heated.
11.	Dashboard; instrumental panel and AC fittings all damaged/burnt/destroyed.
12.	In other words the vehicle is fully burnt and not repairable economically. 

