1.	Load Body/Cabin:- Totally damaged – Not repairable. 
2.	Cowl Assy.:- Show/Cowl assy. totally damaged/dented/deshaped.
3.	Chassis Frame:- Badly bent/twisted. It cannot be repaired.
4.	Engine Assy.:- The Engine assy. is damaged; alternator damaged; self damaged & engine foundations broken.
5.	Front Suspension:- Front Suspension of the vehicle got separated from the chassis frame. Shackle/Hanger assys. broken; U/C Bolts bent; Spring leaves assys. distorted/bent/broken; tie rod long; small; link rods bent; tie rod ends broken; brake pipes bent.
6.	Rear Suspension:- Rear Suspension assy. broken from the chassis frame. Hanger/Shackle assy. broken; U/C Bolts bent; Spring leaves assy. distorted/bent. 
7.	Electrical System:- Meter panels along with Meters broken; wiring completely broken; Switch broken.
8.	Brake System:- Brake System totally damaged.
9.	Battery:- broken.
10.	Diesel Tank:- Dented/deshaped – Diesel Pipes bent.
11.	While inspecting the vehicle, it was observed that the alternator fixed with the engine, fan belt, water body, chamber are dented/damaged. Some other damages can came to light when the engine is taken out. I am taking in consideration the value of those parts which can damage in the engine assy. Gear box, which please note.

The vehicle is lying at Telli Colony, Bari-Brahmana, Distt. Samba, J&K.
